## Intersection of http://hl7.org.au/fhir/StructureDefinition/au-location and http://hl7.org.au/fhir/StructureDefinition/au-location

This is the set of resources that conform to both AU Base Location (http://hl7.org.au/fhir/StructureDefinition/au-location) and AU Base Location (http://hl7.org.au/fhir/StructureDefinition/au-location).

### Structure

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Location |  | 0..* |  | A location in an Australian healthcare context dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated dom-5: If a resource is contained in another resource, it SHALL NOT have a security label dom-6: A resource should have narrative for robust management
meta | Σ | 0..1 | Meta | Metadata about the resource ele-1: All FHIR elements must have a @value or children
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created ele-1: All FHIR elements must have a @value or children
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
ele-1: All FHIR elements must have a @value or children
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation ele-1: All FHIR elements must have a @value or children
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
identifier | Σ | 0..* |  | Unique code or number identifying the location to its users ele-1: All FHIR elements must have a @value or children
status | ?!Σ | 0..1 | code | active | suspended | inactive Binding: ?? (required): Indicates whether the location is still in use. ele-1: All FHIR elements must have a @value or children
operationalStatus | Σ | 0..1 | Coding | The operational status of the location (typically only for a bed/room) Binding: ?? (preferred): The operational status if the location (where typically a bed/room). ele-1: All FHIR elements must have a @value or children
name | Σ | 0..1 | string | Name of the location as used by humans ele-1: All FHIR elements must have a @value or children
alias |  | 0..* | string | A list of alternate names that the location is known as, or was known as, in the past ele-1: All FHIR elements must have a @value or children
description | Σ | 0..1 | string | Additional details about the location that could be displayed as further information to identify the location beyond its name ele-1: All FHIR elements must have a @value or children
mode | Σ | 0..1 | code | instance | kind Binding: ?? (required): Indicates whether a resource instance represents a specific location or a class of locations. ele-1: All FHIR elements must have a @value or children
type | Σ | 0..* | CodeableConcept | Type of function performed Binding: ?? (extensible) ele-1: All FHIR elements must have a @value or children
telecom |  | 0..* | ContactPoint | Contact details of the location ele-1: All FHIR elements must have a @value or children
address |  | 0..1 |  | Physical location ele-1: All FHIR elements must have a @value or children
physicalType | Σ | 0..1 | CodeableConcept | Physical form of the location Binding: ?? (preferred) ele-1: All FHIR elements must have a @value or children
position |  | 0..1 | BackboneElement | The absolute geographic location ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
longitude |  | 1..1 | decimal | Longitude with WGS84 datum ele-1: All FHIR elements must have a @value or children
latitude |  | 1..1 | decimal | Latitude with WGS84 datum ele-1: All FHIR elements must have a @value or children
altitude |  | 0..1 | decimal | Altitude with WGS84 datum ele-1: All FHIR elements must have a @value or children
managingOrganization | Σ | 0..1 | Reference(Organization) | Organization responsible for provisioning and upkeep ele-1: All FHIR elements must have a @value or children
partOf |  | 0..1 | Reference(Location) | Another Location this one is physically a part of ele-1: All FHIR elements must have a @value or children
hoursOfOperation |  | 0..* | BackboneElement | What days/times during a week is this location usually open ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
daysOfWeek |  | 0..* | code | mon | tue | wed | thu | fri | sat | sun Binding: ?? (required): The days of the week. ele-1: All FHIR elements must have a @value or children
allDay |  | 0..1 | boolean | The Location is open all day ele-1: All FHIR elements must have a @value or children
openingTime |  | 0..1 | time | Time that the Location opens ele-1: All FHIR elements must have a @value or children
closingTime |  | 0..1 | time | Time that the Location closes ele-1: All FHIR elements must have a @value or children
availabilityExceptions |  | 0..1 | string | Description of availability exceptions ele-1: All FHIR elements must have a @value or children
endpoint |  | 0..* | Reference(Endpoint) | Technical endpoints providing access to services operated for the location ele-1: All FHIR elements must have a @value or children
Documentation for this format