AU Base Implementation Guide
7.0.0-ballot1 - Ballot

AU Base Implementation Guide - Downloaded Version 7.0.0-ballot1 See the Directory of published versions

## Example Endpoint: Endpoint - a secure messaging endpoint example

Page standards status: Informative

Profile: AU Base Endpoint

> HL7 V2 Receiving Facility

> - namespace-id: CIB
> - universal-id: 877F9695-1298-4E6A-B432-0FDD46AD80B8
> - universal-id-type: GUID

> HL7 V2 Receiving Application

> - namespace-id: Argus
> - universal-id: Argus:7.6.0
> - universal-id-type: L

Encryption Certificate PEM X509: -----BEGIN CERTIFICATE----- -----END CERTIFICATE-----

identifier: `http://example.org/endpoint-identifier`/Argus SupportUnknownL, `http://ns.electronichealth.net.au/smd/target`/http://ns.argusdca.com.au/smd/id/hostname/ACC5959010000000

status: Active

connectionType: Endpoint Connection Type AU: http://ns.electronichealth.net.au/smd/intf/SealedMessageDelivery/TLS/2010 (Sealed Message Delivery)

name: Telstra Health Secure Messaging Endpoint

managingOrganization: Telstra Health

contact: cib@argus.example.net

period: 2017-08-18 --> (ongoing)

payloadType: Simplified Profile for HL7 V2.4 REF message, HL7 V2 MDM Discharge Summary

payloadMimeType: application/hl7-v2

address: https://uatsmd.connectingcare.com/cc.smd/SealedMessageDelivery.svc